Technical Bulletin

To: Per Distribution List From: Scott Hudanish Date: 12/06/10

 Subject: ADS1 Vortex Revision

***Bulletin 120610- Internal Bulletin***

***This bulletin is being issued to ITW Dynatec Internal Personnel.***

The ADS1 Dynafill Hopper Filler Vortex Inlet has recently undergone some revisions to improve the performance of the filler system and provide customer safety awareness.

Vortex Inlet Connection

The Vortex Inlet Vent connection has been revised to add 5 degrees of angle increase to the feed hose connection and lowered the connection .250” inches from the top of the inlet housing. This revision should eliminate or reduce the emission of dust from the Vortex Filter Cap.

Customer Safety

The Vortex Filter Cap will be affixed with a Warning Hot Sign on top of the Vortex assembly.

The following page illustrates and identifies these changes..

****